# tscinbunyTutorial

<a href="https://tscinbuny.com/" target="_blank">https://tscinbuny.com/</a>

>> ESP32 S3 PLUS 
>> Arduino UNO R4 MINMA


## Development Board for Arduino UNO ESP32 Programming Learning

<a href="https://tscinbuny.com/products/tscinbuny-development-board-for-arduino-uno-esp32-programming-learning-controller" target="_blank">바로가기</a>

<img src="https://cdn.mkaidevops.xyz/tscinbuny/ArduinoUNO_ZYZ0366_1.webp" width="480" height="360"/>
<img src="https://cdn.mkaidevops.xyz/tscinbuny/ArduinoUNO_ZYZ0366_2.webp" width="480" height="360"/>
<img src="https://cdn.mkaidevops.xyz/tscinbuny/ArduinoUNO_ZYZ0366_3.webp" width="480" height="360"/>
<img src="https://cdn.mkaidevops.xyz/tscinbuny/ArduinoUNO_ZYZ0366_4.webp" width="480" height="360"/>
<img src="https://cdn.mkaidevops.xyz/tscinbuny/ArduinoUNO_ZYZ0366_5.webp" width="480" height="360"/>

### Description

Tscinbuny Development Board for Arduino UNO ESP32 Programming Learning Controller

Product parameters:

1. Programming software: Arduino IDE
2. Voltage: 7.2~8.4V
3.  ESP32-S3-WROOM-1-N16R8 module and Renesas P7FA4M1AB3CFM#AA0 microcontroller are adopted.
4. Built-in ESP32-S3 series SoC, Xtensa® dual-core 32-bit LX7 microprocessor
5. 16MB Flash, 8MB PS RAM, 384kB ROM
6. 36 GPIO ports
7. On-board PCB antenna, support external antenna
8. Support 802.11b/g/n standard 2.4GHz Wi-Fi, Bluetooth 5.0
9. Data rate 150Mbps
10. ADC, GPIO, I²C, I²S, SPI, PWM, UART, USB
11. Operating Temperature -40°C ~ 65°C (TA)
12. Communication mode: UART/WIFI
13. Product Size: 20cm*13cm*4.5cm
14. Weight 553g